1.Upgrade the ss928-input or ss928-output

Upgrade either ss928-input or ss928-output based on the current node status. For example, upgrade ss928-input when the node is in encoding mode, and upgrade ss928-output when the node is in decoding mode.

2.Upgrade the patch_ss927 and patch_kvm


3.after upgrade all three firmware files,restart the devices










